**ASSEMBLY AND INSTALLATION INSTRUCTIONS**

**WARNING: SHUT POWER OFF AT FUSE OR CIRCUIT BREAKER!**

**NOTE: BEFORE INSTALLING, CONSULT LOCAL ELECTRICAL CODES FOR WIRING AND** **GROUNDING REQUIREMENT**.

**Installation Steps:**

1. Shut off the power at the circuit breaker box. Remove old fixture and all hardware from Outlet Box.
2. Carefully unpack your new fixture and lay out all the parts on a clear area. Take care not to lose any small parts necessary for installation.
3. This product does not include any shades. Shades are sold separately.
4. Hold the Mounting Plate up against ceiling Outlet Box, aligning the Outlet Box two thread holes and adjust to the appropriate location, use a pencil to mark the Wood Screw holes, remove the Mounting Plate, then drilled holes and loaded Plastic Anchors. Attach the Mounting Plate to the Outlet Box with the two Outlet Box Screws and two Wood Screws as shown. The side of the Mounting Plate marked "GND" must face out.
5. This Lamp Body includes 2 sets(16pcs) of Pipes to be connected into various heights. Measure and determine correct number of pipes required. Feed the wires through Pipes and Joint, connect the Pipe to the top thread nipple of the Lamp Body. Thread the thread nipple to inside of each Pipes, connect all the Pipes and Joint together until secure. Raise the Canopy, Spring Shim onto the thread nipple of Joint, lock them securely with Wing Nut.
6. Take the Lamp Body assembly to ceiling Outlet Box, connect the electrical wires**.**
7. **NOTE: make wires connections:**

**\*\*Attach fixture ground wire to supply ground wire using a wire nut or** **attach them to the mounting plate with a green ground screw.**

**\*\*****Attach fixture white wire from lamp body to supply white wire or ridge wire from power source with a wire nut.**

**\*\*Attach fixture black wire from lamp body to supply black wire or smooth wire from power source with a wire nut.**

**\*\*Observing: positive wire with positive wire, negative wire with n****egative wire, ground wire with ground wire.**

1. Make sure all wire connectors are secured and do not easily pull off with the slight tug. After wires are connected, tuck them carefully inside the Outlet Box. Raise the Canopy on to the Outlet Box, align the mounting holes of side with mounting thread holes in mounting plate and lock it securely with the Mounting Screws.
2. Install the light bulbs (Not included) in accordance with the fixture’s specifications.

**NOTE: DO NOT EXCEED THE MAXIMUM WATTAGE RATING!**

1. Your installation is now complete. Return power to the outlet box and test the lamp body.

1955-3XX